第一种刷机方式：USB 线刷 
 
需要准备的刷机硬件：电脑，USB 线 
1， 首先下载刷机工具和驱动 DriverAssitant_v4.4  and FactoryTool-v1.43e   下载链接： 
2， 解压驱动安装包[image: ]和刷机工具安装包 ，
出现
和

 
[bookmark: _GoBack]首先点击打开驱动文件夹（DriverAssitant_v4.4），选择 DriverInstall 安装驱动，如下图所示， 
[image: ] 
 
 
3，打开并弹出对话框，点击驱动安装，显示安装完成，如下图所示 
[image: ] 
 
 
 
 
 
 
4，双击打开文件夹刷机工具（FactoryTool-v1.43e ），点击 FactoryTool，如下图所示， 
[image: ] 
 
 
 
 
5，弹出对话框， 如下图所示 
[image: ] 
 
 
 
 
 
6，点击 Firmware，找到下载的软件位置，选择并点击 Open ,如下图所示 
[image: ] 
7，点击 RUN，等待 Upgrade Prompt 加载，如下图所示， 
[image: ] 
 
8，等待 Upgrade Prompt 加载 100%并显示 Success，完成刷机，如下图所示，




 

	                 





 
第二种刷机方法
需要准备的刷机硬件：SD 卡 
[image: ]  
1， 将下载好的刷机固件拷入 SD 卡根目录 
2， 首先开机进入系统，然后将 SD 卡按压插入机器，如图所示 
[image: ] 
3，插入后，弹出对话框，选择 Install 如图所示 
[image: ] 
 
 
 
 
3， 加载完成，会弹出 checking the package! the device is going to reboot...Do NOT remove SD card from the device 
[image: ] 
 
4， 重启开始加载升级中，直到进入系统，完成刷机 
[image: ] 
 
image17.jpg




image20.jpg
DriverAssitan!
tvad




image30.jpg
FactoryTool-
Vid3e




image5.jpg
A | > DriverAssitant vA4

Neme
s Quick access
i Desktop.

s Downloads

© ADEDriver
* bin

© Diver
 Log

41 config

S, Driverlnstall

LR

oSt
1 Screenshots

BiAN= Application Tools

DriverAssitant_vA.4

Date modified

10/8/2015 %:18 AM
10/8/2015 9:18 AM
10/30/2015 525 PM
3/23/2018 .27 PM
6/3/2014338 PM
10/30/2015 526 PM
6/4/2014 344 PM

Type
File folder

File folder

File folder

File folder
Configuration sett
Application

Tert Document

Size

1K8
290KE
K8




image6.jpg
[ wamr | wowm

OO





image7.jpg
BN Application Tools

Manage
21 > FactonyTookvie

Name -
s Quick access

% bin
mDskop

¥ Language
s Downloads * a Log

” 47 config

TPwes 4 R Factorylool
i
1 FAQ
36t

1 Screenshots

¥ OneDrive

FactoryTool-

Date modified

1/8/2016 516 PM
1/8/2016 516 PM
3/23/2018 .28 PM
11/10/2017 917 AM
1/11/2017 400 PM

Type
File folder

File folder

File folder
Configuration sett.
Application

Size

4K
1,626 K8




image8.jpg
Wi FactoryTool v1.43

Device List DeviceType | 1D
8 My Computer
ootHub20
% Port[1]
% Port[2]
% Port[3]
% Port[4]
% Port[5]
% Port[6]
% Port[7]
% Port[8]
% Port[9]
% Port{10]
% Port{11]
% Port{12]
% Port{13]
% Port{14]
% Port{15]
% Port{16]
% Port{17]
% Port{18]

Fizard:

1.First use, Tag USB port:plug device in,record ID shoving on the tool.Tag all.

2.After pluging device in,comect another until device is doing upgrade.
3.1ed is green,plug device iniled is red,do not plug device in or out.

4.After finishing upgrade, green to show success,red to show failure.

) e o

Firmvare Ver:
Loader Ver:

Chip.

Upgrade Prompt

5.To show successful device on the right of grid and failed device on the left of grid.

D
>
Success
Fail
Total

Success

00000

00000

00000





image9.jpg
W FctonToo

5.To show successful device on the right of grid and failed device on the left of grid.

= B w0
Firmrare Ver
Firmvare | ]
Loader Ver \
bens | | cmn
D W Open X
« ~ 4 [ > ThisPC > Desktop > E > TVBOX > Al > 709NO vo »
Organize = New folder
A Neme Date modified Type size
# Quick access o
A1_709N0_20180127 323/2018619AM  DiscimageFile 1656383 KE
M Desktop e T 9 1656/
& Downloads #
Documents #
& Pictures #
ma
[
@ 6st
] Screenshots
[ OneDrive
SDXC (0
Vizard: kS
o Network v
LFirstul _ _
2. 4¢ter p File name: | A1_709N0 20180127 | | Firmware(*.img)/LoaderC"bin) ~
3.1ed is Open Cancel
4. After fINTSMINE UDETAUE; TYEEN TO SHOW SUCCESS; T To SHOWTaITUrer ey 00000





image10.jpg
Wi FactoryTool v1.43 -

U P Y )

Firmware [C-\Users administzator Deskiop B 578 TRV B00AL 1000 AL 1SN0 20160127, iad | Firmware Ver:7.1.00
Loader Ver:2.43 5

mo | -

Device List DeviceType | 1D Upgrade Prompt

=8 My Computer .
ootHub20

& Port[1]

+ Port[2] Loader 6 Download Firmware(12%).

% Port[3]

% Port[4]

% Port[5]

% Port[6]

% Port[7]

% Port[8]

% Port[9]

% Port{10]

% Port{11]

% Port{12]

% Port{13]

% Port{14]

% Port{15]

% Port{16]

% Port{17]

% Port{18] v

Fizard:

1.First use, Tag USB port:plug device in,record ID shoving on the tool.Tag all. success: 00000

2.After pluging device in,comect another until device is doing upgrade.

Fail 00000

3.1ed is green,plug device iniled is red,do not plug device in or out.
4.After finishing upgrade, green to show success,red to show failure.

Total 00000

5.To show successful device on the right of grid and failed device on the left of grid.





image11.jpg
w

® 0 -]

Firavare [C\Users\Adainistrator Desktop B 78 TEVIV BONAL\T0SNO\ALT08N0_Z0160127.

oo ||

Device List DeviceType | 1D
8 My Computer
ootHub20
% Port[1]
% Port[2]
% Port[3]
% Port[4]
% Port[5]
% Port[6]
% Port[7]
% Port[8]
% Port[9]
% Port{10]
% Port{11]
% Port{12]
% Port{13]
% Port{14]
% Port{15]
% Port{16]
% Port{17]
% Port{18]

Fizard:

1.First use, Tag USB port:plug device in,record ID shoving on the tool.Tag all.

2.After pluging device in,comect another until device is doing upgrade.
3.1ed is green,plug device iniled is red,do not plug device in or out.

4.After finishing upgrade, green to show success,red to show failure.

- @ =]

Firmvare Ver:7.1.00

Loader Ver:2.43

Chip: RK322H

Upgrade Prompt

5.To show successful device on the right of grid and failed device on the left of grid.

N

D Success

success: 00001

Fail 00000

Total 00001





image12.jpeg
w

® 0 -]

Firavare [C\Users\Adainistrator Desktop B 78 TEVIV BONAL\T0SNO\ALT08N0_Z0160127.

oo ||

Device List DeviceType | 1D
8 My Computer
ootHub20
% Port[1]
% Port[2]
% Port[3]
% Port[4]
% Port[5]
% Port[6]
% Port[7]
% Port[8]
% Port[9]
% Port{10]
% Port{11]
% Port{12]
% Port{13]
% Port{14]
% Port{15]
% Port{16]
% Port{17]
% Port{18]

Fizard:

1.First use, Tag USB port:plug device in,record ID shoving on the tool.Tag all.

2.After pluging device in,comect another until device is doing upgrade.
3.1ed is green,plug device iniled is red,do not plug device in or out.

4.After finishing upgrade, green to show success,red to show failure.

- @ =]

Firmvare Ver:7.1.00

Loader Ver:2.43

Chip: RK322H

Upgrade Prompt

5.To show successful device on the right of grid and failed device on the left of grid.

N

D Success

success: 00001

Fail 00000

Total 00001





image12.jpg
468

me3
==e




image13.jpg




image14.jpg
AppMarket

Gallery.

e N gt

Bee Files Explorer Bee Music Calculator Camera Chrome Downloads
A Firmware Updating <
Media Center WifiDisplay

A update package file is found : '/mnt/media_rw/BAED-07E5/
update.zip'. Would you like to install the package?

concel _




image15.jpg
@ ™ " %

AppMarket Bee Files Explorer Bee Music Calculator Camera Chrome Downloads

Gallery Media Center £\ Firmware Updating WifiDisplay

Checking the package! The Device is going to reboot...Do NOT
remove SD card from the device!




image16.jpg
Installing system update




image1.jpg




image2.jpg




image3.jpg
DriverAssitan!
tvad




image4.jpg
FactoryTool-
Vid3e




