How to use the PVE version screen software  

1. Unzip the file, enter the AOOSTAR-X-linux folder, right-click on the blank space, open in terminal or cd to the AOOSTAR-X-linux directory.
Note: The path cannot contain special symbols or Chinese characters.

2、Install and start the service by entering the following in the terminal: (root privileges and password required)
[bookmark: _GoBack]
# PVE requires the following additional commands to run
apt update
apt install sudo

# Startup screen software
chmod +x ./create_service.sh
sudo ./create_service.sh

3、Install lm-sensors + it87 driver (displays fan speed and other sensor information; installation is not mandatory)

# Install lm-sensors
sudo apt update
sudo apt install lm-sensors

# Install dependencies
apt update && apt install -y pve-headers proxmox-headers-$(uname -r) dkms flex bison

# install it87
dpkg -i it87-dkms_1.0.63-1_all.deb

Note: If you encounter errors that require resolving dependencies or conflicts, please refer to the following:

# Uninstall lm-sensors
sudo apt remove lm-sensors


===================================================================================================================

HOW to use the Unraid version screen software  

1、Unraid web backend—>APP—>Search—>User Scripts—>Install, return to Unraid web backend—>APP—>Search—>ITE IT87 Driver—>Install

2、Upload the AOOSTAR-X-linux folder to the array directory (e.g., mnt/disk1: uploading to another directory will cause a reboot and reset). After uploading, the path should be mnt/disk1/AOOSTAR-X-linux/AOOSTAR-X.

3、Connect to Unraid via SSH，cd mnt/disk1/AOOSTAR-X-linux

4、chmod +x AOOSTAR-X

5、Unraid web backend—>Apps—>Installed apps—>User Scripts—>More actions—>Settings—>ADD NEW SCRIPT—>Enter “STAR-AOOSTAR-X”—>OK

6、Click the gear icon to the left of “STAR-AOOSTAR-X” -> EDIT SCRIPT -> Enter the following content:

#!/bin/bash
cd /mnt/disk1/AOOSTAR-X-linux && nohup ./AOOSTAR-X > aoostar.log 2>&1 &

7、Click “SAVE CHANGES” to save—>Change “Schedule Disabled” to “At Startup of Array”—>APPLY

8、Unraid web backend—>Settings—>Hard Disk Settings>Enable Auto Start—>Change to ‘Yes’

===================================================================================================================

Screen software installation steps for WINDOWS system versions

Double-click AOOSTAR-X-Setup.exe to install. Windows or Windows Server must have all drivers installed, otherwise the software will report an error and fail to start.


# General description:

The background port is 5123, and the default username and password are admin and 123456. Please change the password promptly to avoid security risks.


