The instruction to flash BOIS via USB flash disk.

1. Please unzip the “BOIS”and copy all the files in BOIS to the root directory of the USB flash disk.

2. Please format the USB flash disk into the format of “FAT32”and rename it as “WINPE”.

3.The picture is the reference, the BIOS file is based on the actual downloaded BOIS file.
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4. Please put the USB flash disk and USB keyboard to the tablet. Make sure that the tablet is off and then press the power button, at the same time, please click the “F7”continuously to enter the boot mode.
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5.Choose “UEFI:Generis,Partition 1”to click “enter”. When the BIOS is finished flashing, please take off the USB flash disk to avoid flashing BOIS again.
[image: ]


image1.png
=5

befi

[ afuefi

] afuefixsaefi
@sios

] C106_B101UAN.rom
[ startupnsh

BHES

2016/1/27 14:33
2016/1/27
2016/1/27 14
2016/1/26 17:23
2016/1/26 17:23
2016/1/27

B~
St

EFL0f
BIN 30t
R
NSH 3276

ESN

7x8
368 K8
81028
6,345 K8
1K8




image2.png
Plese selct tont dvice:

Hindous oot Knager
(EFL: Gerric, Patition 1
Eter Setwp

T o e selection
ENTER to slect boot deice
ESC to bot using deflts





image3.png
oo o s +483 NO108 To

PCiR00t (0x0) /Pei (0x1:
B %10,0%0) /Ctp,

o 0
blk3
blk4
BIKS  :HardDisk - Allas (null)
PEiR001 (0x0) /PC i (0x10, 0%0) /CtrL (0x0) 4608 :
,0%8000)
bk6  :BlockDevice - Allas (nuLl)
F(lRDDt(OXO'/PCJ(0¥J(I,0X0)/C(PJ(O<O)
blk7? :BlockDevice - Alias (null)
PCiR00t (0%0) /Pci(0x10,0%0) /Ctrl(0x1)
blks :BlockDevice - Alias (null)
PCiR00t (0x0) /Pci(0x10,0x0) /Ctr1(0x2)
blkg :Removable BlockDevice - Alias (null)

PCiR00t (0%0) /PC1(0x14,0%0) /USB(0x3, 0%0)

ress ESC in 4 seconds to skip startup.nsh, any other key to continue

AMI Firmuare Update Utility v5.08.00
Copyright (C)2015 American Megatrends Inc. ALl Rights R

Reading flash . done

- ME Data Size checking . ok :
cure Flash enabled, recalculate ROM size with signature... Enabl:

- FFS checksums ......... ok

Loading capsule to secure memory buffer ... done

00388000 (63%)





