1. Unzip the file and put it in the root directory of the USB drive
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[bookmark: _GoBack]2. Insert the USB drive into the machine, press F7 to enter the flash disk boot interface, select the USB drive and press Enter to start upgrading the BIOS.[image: ]3. Do not cut off the power during the BIOS upgrade. The machine will automatically shut down after the upgrade. Unplug the USB drive and restart the machine.
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Please select boot device:

Mindows Boot Manager (FCN006-5126 550)

UEFI: Teciast CoolF lash USE3.01100, Pertition 1 (Teclast CoolFlash USB3.O1:
enter setup

7 and 4 to move selection
ENTER t0 select boot device
ESC to boot using defauits
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Mapping table o :
: i :HDONOb: ;BLK1: < B95D
e Pgi;gzsz)xo)m:i (6x14 ,0%0) /USB(0xD,0x0) /HD(1,HBR, O.
0000)
FS1: Alias(s) :HDONOC: ;BLK2:

PCiR00t (0x0) /Pci(0x14,0x0) /USB(OXD,0x0) /HD (2, MBR , 0xBI3DE
x6D2F000)

FS2: Alias(s):HD1ib:;BLK4:

PciRoot(oxo)/Pci(oxiD,Oxs)/Pci(Ox0,0xO)/NVMe(Oxl,06—04—0(

3A) /HD(1,GPT, 1C643F95- 188A-43C2-A708-00D091C7B278 > 0xX800,0x32000)
FS3: Alias(s):HD1d:;BLKs:

PciRoot(Oxo)/Pci(Oxlo,OXSJ/Pci(Oxo,0x0)/NVHe(0x1,06—04—00
SA)/HD(S,GPT,239334DD-251C—42E5—RE3E

—45303E12FF4D,0x?2800,0x3558800
FSq: Alias(s) :HD1e:;BLK7:

PciRoot(Oxo)/Pci(0x10,0x3)/Pci(0x

0,0x0)/NVHe(0x1,06—04—00—
39)/HD(4,GPT,DsaS1143—1?6E-4550-9230—02E3ﬂﬂ99758F,oxSBSZRBOO,OXSBSBO
BLKO: Alias(s):

PciRoot(oxo)/Pci(ox

14,0x0)/USB(0xD,0x0)
BLK3: Alias(s):

PCiR:
. C i oot(Oxo)/Pci(OxlD,0x3)/Pci(Ox0,0xO)/NVNe(Oxl,06—04—00—1
BLKS: Alias(s):
PclRoot(OxO /P
T ) Ci(0x1D,0x3

)/Pci(oxo 0x%0) #N
,GPT,DEE4F259-DDO:3-45A5-B7F o s VMe (0x1, 06-049-00- 1,
C 1 seconds 1o akip starf 3?73Fc1a1sas,0xszaoo,0xqoooo)
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