FLASH BIOS


①：Under “uefi shell” flash BIOS
[bookmark: _GoBack]②：Under “Windows” flash BIOS
Prepare: USB Disk*1----32GB and more than
Software: rufus
1、Open software “rufus”，boot symbol is “ms-dos” click “start”
[image: ]
2、Extract the file and place it in the root directory of the USB disk
[image: ]
3、Insert USB disk into the computer‘s USB PORT

4、Power computer press F7

5、Selection UEFI :USB DISK

6、Into “shell” will l auto flash BIOS）pay attention to：the flashing process cannot be powered off or shut down
[image: ]
7、FLASH  successful

8、Discover the power adapter first，then plug in the adapter and power it on to startup
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