FLASH BIOS

Method 1:under “uefi shell” flash BIOS

Method 2:“Windows” flash BIOS 

Prepare: USB Disk*1----32GB and more than

software ：rufus

Method 1：Under “uefi shell” flash BIOS

create the bootable USB drive

Insert USB drive and open software “rufus”，Boot selection is “MS-DOS”,click “START”.
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2.Extract the BIOS file and place it in the root directory of the USB disk.
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3.Plug the prepared USB drive into the computer’s USB port for BIOS flashing.
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4.After plugging in the computer and turning it on, press "F7" repeatedly on the keyboard
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5.Selection UEFI :USB DISK
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6.Into “shell” will auto flash BIOS

Pay attention to：The flashing process cannot be powered off or shut down
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7.FLASH  successfu
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8. Locate the power adapter, unplug it, plug it back in, and then power on the device.
Method 2：Under “Windows” flash BIOS 


1.Extract the BIOS file into the desktop
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2.Double-click left button ，run “Win Flash”
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Waiting flash over，press any key continue 

pay attention to：the flashing process cannot be powered off or shut down
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4.Shut down first and then upplug the adapter，and plug adapter power on
