
1.Prepare a U disk（USB flash drive）  with a storage capacity of at least 16 GB.

[bookmark: _GoBack]2.Right click and select format... Format U disk to FAT32 format,and change the
Volume label to WINPE ,click start to finish formatting.
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3.Copy the files to U disk as below, and it must be in the root directory of U disk.
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4.Restart the computer, press F7 repeatedly on  the boot logo interface, and select
USB boot in the boot options.
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5.After then,please wait for it flash automatically until it complete.
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[image: ]6.Please enter exit.
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