第一种刷机方式：USB线刷
需要准备的硬件：电脑，USB线
1， 下载刷机工具PhoneixUSBPro_V_4_0_0__2014-09-12EN
下载链接：
https://beelink-my.sharepoint.com/:u:/g/personal/firmwareservice_beelink_onmicrosoft_com/EccEJ1Rac4ZBsDEPp0-gkxABx2WRv682NvN1BHq27WAtsA?e=23JIke

2， 解压安装包[image: ] 右击解压到当前文件夹后，出现图标软件[image: ]，双击打开进行安装，如下图所示，一直点击Next 安装软件
[image: ]



3， 安装完成，双击打开桌面软件图标[image: ]，如下图所示
[image: ]










4， 加载固件，点击Image, 找到下载的软件位置，选择并点击Open ,如下图所示
[image: ]











5， 将USB一端插入电脑USB接口，
A：用小针按下机器后面的小孔，不要移动
B：然后将USB另一端插入HDMI旁边的USB接口
[image: ]

6， 继续按住，等待30秒以上
7， 等待[image: ]变成绿色模式，如下图所示
[image: ]


8， 进度100%后，拔掉，完成刷机
[image: C:\Users\Administrator\Desktop\FAQ\GS1\QQ图片20180322111855.png]










第二种刷机方式：SD/USB本地升级方式

需要准备的硬件：SD卡/USB U盘
1，点击图标[image: ]，进入setting
[image: ]
2，点击About TV Box
[image: ]
3，点击System Recovery
[image: ]
4，弹出如下图对话框，点击Select file
[image: ]






[bookmark: _GoBack]5，找到SD卡 or USB U盘，找到本地升级固件，选择并确定
[image: ]
[image: ]
6，开始加载Verifying….
[image: ]


7，完成Ready to reboot
[image: ]
9， 自动重启，开始升级Installing system update,
完成刷机
[image: C:\Users\Administrator\Desktop\FAQ\GS1\QQ图片20180322113508.png]
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Welcome to the PhoneixUSBPro Setup Wizard (r7

The installer vill guide you through the steps required to install
Phonei xUSEPro on your coaputer.

VARNING: This coaputer progran is protected by copyright lav and
international treaties. Unauthorized duplication or distribution of
this progras, or any portion of it, may result in severe civil or
crininal penalties, and vill be prosecuted to the aaxima sxtent
possible under the lav.





