There are two ways to refresh the BIOS.

The first method: double-click AFUWINx64.EXE to refresh the BIOS directly.

The second method: use a USB flash drive to refresh the BIOS.
Step 1: Format the USB flash drive into FSTA32 format;
Step 2: Unzip the BISO to the root directory of the USB flash drive;
Step 3: Turn off the machine. Then restart the machine, and keep pressing F7 to enter the USB flash drive boot;
[bookmark: _GoBack]Step 4: After entering the USB flash drive boot, select the UEFI option, select it and press Enter, and you will enter the BIOS installation interface. After completing the subsequent steps, the machine will automatically shut down or restart after the installation is completed.
